
 SAFETY DATA SHEET 
1. IDENTIFICATION OF THE SUBSTANCE/ PEREPARATION AND OF THE COMPANY / UNDERTAKING 
Product Name Red Rouge Polishing Compound 
Recommended use of the chemical and restriction on use 
Recommended Use Abrasive/ Buffing Compound 
2. HAZARDS IDENTIFICATION 
Classification 
This item is not considered hazardous by the 2012 OSHA Hazard Communication Standard (29 CFR 1910.1200) 
This product is a pre-molded cake form Red with a tallow odor 
GHS Label elements, including precautionary statement 
EMERGENCY OVERVIEW 
Signal Word None 
Hazard Statement None 
The products/products contain no substances which at their given concentration are considered to be hazardous to health. 
Appearance: Premolded Cake Form Physical State: Solid Odor: Tallow Odor 
Precautionary Statements – Prevention 
Obtain Special Instructions before use 
Other information 
May cause slight eye irritation 
Prolonged or repeated contact may dry skin and cause irritation. 
Interaction with other chemicals 
No information available 
3. COMPOSITION / INFORMATION ON INGREDIENTS. 
Red Rouge 
Chemical Name CAS No. % 
Aluminum Oxide 1344-28-1 68-75 
Stearic Acid 134503-33-6 15-20 
Iron Oxide 1309-37-1 8-15 
Tallow 129521-65-9 5-15 
*The exact percentage (concentration) of composition has been withheld as a trade secret 
4. FIRST AID MEASURES 
Eye Contact: Rinse thoroughly with plenty of water, also under the eyelids. If symptoms persist, call a physician. 
Skin Contact: Wash skin with soap and water. In the case of skin irritation or allergic reactions see a physician. 
Inhalation: Remover to fresh air. If symptoms persist, call a physician. 
Ingestion: Do NOT induce vomiting. Drink plenty of water. If symptoms persist, call a physician. 
Most important symptoms and effect, both acute and delayed 
Most important symptoms and effect No information available 
Indication of any immediate medical attention and special treatment needed 
Notes to Physician Treat symptomatically. 
5. FIRE FIGHTING MEASURES 
Suitable Extinguishing Media 
Use extinguishing measures that are appropriate to local circumstances and the surrounding environment. 
Unsuitable Extinguishing Media 
CAUTION: Use of water spray when fighting fire may be inefficient. 
Specific Hazards Arising from the Chemical 
No information available. 
Hazardous Combustion Products 
Carbon oxides. 
Explosion Data 
Sensitivity to Mechanical Impact No. 
Sensitivity to Static Discharge No. 
Protective equipment and precautions for firefighters 
As in any fire, wear self-contained breathing apparatus pressure-demand, MSHA/NIOSH  full protective gear. 
6. ACCIDENTAL RELEASE MEASURES 
Personal precautions, protective equipment and emergency procedures 
Personal Precautions Avoid contact with eyes. 
Environmental Precautions 
Environmental Precautions Refer to protective measures listed in Sections 7 and 8. 
Methods and material for containment and cleaning up 
Methods for Containment Prevent further leakage or spillage if safe to do so. 
Methods for cleaning up Pick up and transfer to properly labelled containers. 
7. HANDLING AND STORAGE 
Precautions for safe handling 
Handling Handle in accordance with good industrial hygiene and safety practice. Avoid contact with eyes. 
Conditions for safe storage, including any incompatibilities 
Storage Keep container tightly closed. 
Incompatible Products None known based on information supplied. 
8. EXPOSURE CONTROLS/PERSONAL PROTECTION 
	Exposure Guidelines: Hazardous Component 
	OSHA PEL 
	ACGIH TLV 

	Aluminum oxide 
	15 mg/m3 TWA (total dust) 
5 mg/m3 TWA (respirable) 
	1 mg/m3 TWA 
(respirable) (as Al) 

	Tallow 
	None Established 
	None Established 

	Iron oxide 
	5 mg/m3 TWA (respirable) 
	10 mg/m3 
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